| IDA SDK

Variables
Color tags
Color definitions

## Detailed Description

Specify a color for a syntax item.

## Variables
const color_t | COLOR_DEFAULT = 0x01
| Default.
const color_t | COLOR_REGCMT = 0x02
| Regular comment.
const color_t | COLOR_RPTCMT = 0x03
| Repeatable comment (comment defined somewhere else)
const color_t | COLOR_AUTOCMT = 0x04
| Automatic comment.
const color_t | COLOR_INSN = 0x05
| Instruction.
const color_t | COLOR_DATNAME = 0x06
| Dummy Data Name.
const color_t | COLOR_DNAME = 0x07
| Regular Data Name.
const color_t | COLOR_DEMNAME = 0x08
| Demangled Name.
const color_t | COLOR_SYMBOL = 0x09
| Punctuation.
const color_t | COLOR_CHAR = 0x0A
| Char constant in instruction.
const color_t | COLOR_STRING = 0x0B
| String constant in instruction.
const color_t | COLOR_NUMBER = 0x0C
| Numeric constant in instruction.
const color_t | COLOR_VOIDOP = 0x0D
| Void operand.
const color_t | COLOR_CREF = 0x0E
| Code reference.
const color_t | COLOR_DREF = 0x0F
| Data reference.
const color_t | COLOR_CREFTAIL = 0x10
| Code reference to tail byte.
const color_t | COLOR_DREFTAIL = 0x11
| Data reference to tail byte.
const color_t | COLOR_ERROR = 0x12
| Error or problem.
const color_t | COLOR_PREFIX = 0x13
| Line prefix.
const color_t | COLOR_BINPREF = 0x14
| Binary line prefix bytes.
const color_t | COLOR_EXTRA = 0x15
| Extra line.
const color_t | COLOR_ALTOP = 0x16
| Alternative operand.
const color_t | COLOR_HIDNAME = 0x17
| Hidden name.
const color_t | COLOR_LIBNAME = 0x18
| Library function name.
const color_t | COLOR_LOCNAME = 0x19
| Local variable name.
const color_t | COLOR_CODNAME = 0x1A
| Dummy code name.
const color_t | COLOR_ASMDIR = 0x1B
| Assembler directive.
const color_t | COLOR_MACRO = 0x1C
| Macro.
const color_t | COLOR_DSTR = 0x1D
| String constant in data directive.
const color_t | COLOR_DCHAR = 0x1E
| Char constant in data directive.
const color_t | COLOR_DNUM = 0x1F
| Numeric constant in data directive.
const color_t | COLOR_KEYWORD = 0x20
| Keywords.
const color_t | COLOR_REG = 0x21
| Register name.
const color_t | COLOR_IMPNAME = 0x22
| Imported name.
const color_t | COLOR_SEGNAME = 0x23
| Segment name.
const color_t | COLOR_UNKNAME = 0x24
| Dummy unknown name.
const color_t | COLOR_CNAME = 0x25
| Regular code name.
const color_t | COLOR_UNAME = 0x26
| Regular unknown name.
const color_t | COLOR_COLLAPSED = 0x27
| Collapsed line.
const color_t | COLOR_FG_MAX = 0x28
| Max color number.
const color_t | COLOR_ADDR = COLOR_FG_MAX
| hidden address marks. More...
const color_t | COLOR_OPND1 = COLOR_ADDR+1
| Instruction operand 1.
const color_t | COLOR_OPND2 = COLOR_ADDR+2
| Instruction operand 2.
const color_t | COLOR_OPND3 = COLOR_ADDR+3
| Instruction operand 3.
const color_t | COLOR_OPND4 = COLOR_ADDR+4
| Instruction operand 4.
const color_t | COLOR_OPND5 = COLOR_ADDR+5
| Instruction operand 5.
const color_t | COLOR_OPND6 = COLOR_ADDR+6
| Instruction operand 6.
const color_t | COLOR_OPND7 = COLOR_ADDR+7
| Instruction operand 7.
const color_t | COLOR_OPND8 = COLOR_ADDR+8
| Instruction operand 8.
const color_t | COLOR_RESERVED1 = COLOR_ADDR+11
| This tag is reserved for internal IDA use.
const color_t | COLOR_LUMINA = COLOR_ADDR+12
| Lumina-related, only for the navigation band.

## Variable Documentation

## ◆ COLOR_ADDR

const color_t COLOR_ADDR = COLOR_FG_MAX

hidden address marks.

the address is represented as 8digit hex number: 01234567. it doesn't have COLOR_OFF pair. NB: for 64-bit IDA, the address is 16digit.