| IDA SDK

Macros
Instruction feature bits

## Detailed Description

Used by instruc_t::feature.

## Macros
#define | CF_STOP 0x00001
| Instruction doesn't pass execution to the next instruction.
#define | CF_CALL 0x00002
| CALL instruction (should make a procedure here)
#define | CF_CHG1 0x00004
| The instruction modifies the first operand.
#define | CF_CHG2 0x00008
| The instruction modifies the second operand.
#define | CF_CHG3 0x00010
| The instruction modifies the third operand.
#define | CF_CHG4 0x00020
| The instruction modifies the fourth operand.
#define | CF_CHG5 0x00040
| The instruction modifies the fifth operand.
#define | CF_CHG6 0x00080
| The instruction modifies the sixth operand.
#define | CF_USE1 0x00100
| The instruction uses value of the first operand.
#define | CF_USE2 0x00200
| The instruction uses value of the second operand.
#define | CF_USE3 0x00400
| The instruction uses value of the third operand.
#define | CF_USE4 0x00800
| The instruction uses value of the fourth operand.
#define | CF_USE5 0x01000
| The instruction uses value of the fifth operand.
#define | CF_USE6 0x02000
| The instruction uses value of the sixth operand.
#define | CF_JUMP 0x04000
| The instruction passes execution using indirect jump or call (thus needs additional analysis)
#define | CF_SHFT 0x08000
| Bit-shift instruction (shl,shr...)
#define | CF_HLL 0x10000
| Instruction may be present in a high level language function.
#define | CF_CHG7 0x020000
| The instruction modifies the seventh operand.
#define | CF_CHG8 0x040000
| The instruction modifies the eighth operand.
#define | CF_USE7 0x080000
| The instruction uses value of the seventh operand.
#define | CF_USE8 0x100000
| The instruction uses value of the eighth operand.