| IDA SDK

Macros
Flow chart flags

## Detailed Description

Passed as 'flags' parameter to qflow_chart_t.

## Macros
#define | FC_PRINT 0x0001
| print names (used only by display_flow_chart())
#define | FC_NOEXT 0x0002
| do not compute external blocks. More...
#define | FC_RESERVED 0x0004
#define | FC_APPND 0x0008
| multirange flowchart (set by append_to_flowchart)
#define | FC_CHKBREAK 0x0010
| build_qflow_chart() may be aborted by user
#define | FC_CALL_ENDS 0x0020
| call instructions terminate basic blocks
#define | FC_NOPREDS 0x0040
| do not compute predecessor lists
#define | FC_OUTLINES 0x0080
| include outlined code (with FUNC_OUTLINE)

## Macro Definition Documentation

## ◆ FC_NOEXT

#define FC_NOEXT 0x0002

do not compute external blocks.

Use this to prevent jumps leaving the function from appearing in the flow chart. Unless specified, the targets of those outgoing jumps will be present in the flow chart under the form of one-instruction blocks